# External Visual VM

## Purpose

The External Visual VM form allows you to specify the NuPoint Unified Messaging or MiCollab Nupoint UM server parameters for the Visual Voice Mail application.

For more information, see About Visual Voice Mail.

## Field Descriptions

Parameter | Description | Default Value
Visual Voicemail Server Address | Enter the address (IPv4, IPv6 or FQDN) of the NuPoint Unified Messaging/MiCollab Nupoint UM server. IMPORTANT: When the voice mail application for a system is changed from Embedded to NuPoint or vice versa, the MiVoice Business system must be rebooted to align the system and sets to the new voice mail application. Otherwise, inaccurate MWI and other voice mail status indicators may result. Changing the voice mail application is done by entering (or deleting) the address in this field. | Blank
Hunt Group | Enter the hunt group number used for arbitrating audio connections. | Blank