# Personal Ring Groups

## Purpose

Use this form to manage personal ring groups containing members who are:

- programmed as Full Service
  This Service Level indicates that the directory number (DN) is assigned to a standard user and device with full telephony functionality. or Trusted Service
  This Service Level indicates that the directory number (DN) is assigned to a trusted Mitel application that has full telephony service once it registers with the system. Although the DN can be programmed on the same forms as a Full Service user/device, it does not use an IP User License. users

- licensed individually with an IP User license (and possibly an EHDU license).

Alternatively, use the Multi-device User Groups form to manage PRGs containing members who are programmed as Multi-Device
This Service Level indicates that the directory number (DN) is assigned to a user that has only basic telephony functionality (e.g., emergency or attendant calls) until programmed as a member of a Multi-Device user group or suite. The DN does not use an IP User License. However, the group or suite has a Multi-device Users or Multi-device Suites license which one person can use at a time in order to receive full telephony service. users and licensed collectively with a Multi-Device license.

## Field Descriptions

Parameter | Description | Default Value
Personal Ring Groups
Personal Ring Group | Enter a valid prime DN up to seven digits in length to be used as the pilot number for the PRG. The pilot number is the number dialed to access the PRG. See Personal Ring Group Conditions for valid numbers. | Blank
One Busy All Busy | This is a programmable option. If this option is enabled, busy is returned if ONE member in the group is busy. If this option is disabled, then all members of the group are rung if one or more members (but not all members) are busy. | No
Prime Member Name | System-generated, protected field. Indicates the name under which the Personal Ring Group's pilot (prime member) is listed in the telephone directory. If no name exists in the Telephone Directory form for the pilot number, this field is blank. |
Home Element | System-generated, protected field. Indicates the name of the primary element for the PRG, which is the NE name of the local MiVoice Business system. |
Secondary Element | System-generated, protected field. The data in this field is the prime member's secondary element. "Not Assigned" is displayed if resiliency is not enabled on the prime member device. If the primary element fails, the PRG fails over to the secondary element that is displayed in this field. If the secondary element field is blank, the group is resilient but the secondary element name is blank. | Not Assigned
Personal Ring Group Members
Member Index | System-generated, protected field. Indicates the number of the member within the group. |
Number | Enter the directory numbers belonging to the Personal Ring Group. See Personal Ring Group Conditions for valid numbers and the maximum members allowed per group. | Blank
Presence | Allows you to set a group member's presence status to Present or Absent. | Present
Name | System-generated, protected field. Indicates the name corresponding to the directory number, as entered in the Telephone Directory form. If no name exists for the associated directory number the field is blank. |
Home Element | System-generated, protected field. Indicates the name of the primary element for the PRG, which is the NE name of the local MiVoice Business system. |
Secondary Element | System-generated, protected field. The data in this field is the prime member's secondary element. "Not Assigned" is displayed if resiliency is not enabled on the prime member device. If the primary element fails, the PRG fails over to the secondary element that is displayed in this field. If the secondary element field is blank, the group is resilient but the secondary element name is blank. | Not Assigned
Local-only DN | If "True" the pilot number of the Personal Ring Group is a local-only directory number. If "False" it is a cluster dialable number. This field only appears in the form if your system has been migrated to support Remote Directory Number Synchronization. |

Related Topics

- Handoff

- Multiline IP Sets

- Personal Ring Groups

- System Capacity