# Program Mitel IP Appliances

## Before You Begin

- Ensure the DHCP Server has been programmed.

NOTES

- If you wish to program a Mitel IP Appliance with a static IP address, refer to the Technician's Handbook.

- The Class of Service must have both the HCI/CTI/TAPI Call Control Allowed option, and the HCI/CTI/TAPI Monitor Allowed option enabled.

## Programming

To program IP appliances:

1. Multiline IP Sets form
   Complete the Device Type, Prime Directory Number, Prime Line Type, Interconnect Number, and the MAC address (optional) fields.

2. Multiline Set Keys form (Optional)
   Assign a directory number (line appearance) or feature to each key.
   Assign each line appearance a ring type.

3. Multiline Appearance Groups form (Optional)
   Change the ring type at each telephone where this number appears.
   Change the group type from "key system" to "multicall" or vice versa.

4. Default Account Codes form (Optional)
   Create a default account code number that will appear in all SMDR records for the station.

5. Station Attributes form
   Assign a Class of Service, Class of Restriction, and Intercept Number to the directory number of the telephone.
   (Optional) Assign a Default Account Code Index number.

6. Telephone Directory form
   Assign a name, department, and location to all directory numbers in the system.

7. Register the IP telephone (optional).
   -this step is required only if the MAC address was not programmed in the Multiline IP Sets form.

NOTE: If you delete telephones, you must also delete the corresponding directory entries and voice mailboxes.