# Programming Loudspeaker Paging (Analog)

To program loudspeaker paging:

1. Loudspeaker Paging form

- Enter the Zone number and Interconnect Number.

- Ensure that stations that require access to paging are not restricted in the Interconnect Restriction Table.

2. Class of Service Options form

- Enable Individual or All Zone paging at the appropriate stations.

NOTE: Symbol wireless phones cannot receive paging messages and should not have these features assigned in their Class of Service.

3. (Optional) Feature Access Codes form

- Assign a paging access code

OR

- Program a paging key in the Multiline Set Keys form.

4. Reboot the Analog Services Unit to start loudspeaker paging operation.