# BRI (Basic Rate Interface)

## Description

BRI (Basic Rate Interface) is a basic ISDN service consisting of two 64 Kbps channels and a single 16 Kbps channel. This is supported by MiVoice Business with the Quad BRI Framer MMC module

## Conditions and Feature Interactions

None

## Programming

To configure the Quad BRI Framer MMC module for embedded BRI, refer to:

- Program Controller Modules

- Program Embedded BRI Trunks

## Device Support

Not applicable

## Operation

None