# VM Ports

## Purpose

The VM Ports form assigns prime directory numbers and interconnect numbers to all voice mail ports.

Use this form when performing the following tasks:

- Program Embedded Voice Mail

## Conditions

- All available ports must be programmed.

## Field Descriptions

Parameter | Description | Default Value
Port ID | System-generated, protected field. Indicates the card position and circuit used for the associated Mitel telephone. |
Prime Directory Number | Enter a unique internal directory number containing up to seven digits that is assigned to the line circuit. | Blank
Local-only DN | Allows you to specify the directory number as a local-only directory number in a cluster. This field only appears in the form if your system has been migrated to support Remote Directory Number Synchronization. | Not Selected
Interconnect Number | Enter a number from 1 to 64 that references an entry in the Interconnect Restriction Table. | 1
Tenant Number | Enter the number of the port's tenant. | 1 (landlord)