# L2 VLAN SHOW

## Qualifiers:

None

## Purpose:

NOTE: This maintenance command is not applicable to MiVoice Business for Industry Standard Servers (ISS).

Shows the VLAN ID assigned to the embedded L2 switch ports in the CXi, CXi II, MXe, and AX and whether the port is tagged (t) or untagged (u).

## Details:

Ports 1-17 are the external ports.

Port 22 is the RTC
1. Real Time Clock. 2. Real Time Complex. The RTC is a card that is used for the IP phones signaling, and for the ESM, DHCP, FTP and TFTP servers, among others. Call progress, device status and screen updated messages are sent between the IP Phones and the RTC. L2 switch port.

Port 21 is the MIPS port and port 20 is the APC .

VLAN membership is assigned in the System IP Properties and Layer 2 (L2) Switch forms. Use also the L2 Stat Port command for additional information about the L2 ports.

## Example:

### Entry: L2 VLAN SHOW

System Response (for CXi):

1 1 1 1 1 1 1 1 1 1 2 2 2

VLAN 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2

(0001)

(0156) u u u u u u u u u u u u u u u u t t

(3156) t u t t t t t t t t t t t t t t t u u u t u

(4094) t t

----