# VM Network Users

## Purpose

Use this form when performing the following tasks:

- Programming Networked Voice Mail

See also,

- About Networked Voice Mail

- VM Network Servers

## Conditions

IMPORTANT: Data in this form is not propagated by SDS to other nodes in the network/cluster. Any changes must be manually entered in the VM Network Users form at other nodes where necessary.

## Field Descriptions

Parameter | Description | Default Value
PNI | The extension's Primary Node ID. | Blank
Mailbox Number | Enter a mailbox number for this extension. The mailbox number is usually the same as the mailbox subscriber's extension number. Do not use the following numbers: 0 (reserved for operator), or 9 (reserved for directory listing). NOTE: The mailbox length can be changed using the Administrator's Mailbox or the Mailbox Length option in the VM Options form. The maximum length is seven digits (same as the maximum for extension numbers). | Blank
Name | Enter up to a 20-character name to identify the user of the mailbox. Enter the name (first name firsVM Options Use a comma to separate the first and last names. The comma does not count as a character. Spaces are not allowed. This parameter can also be changed using the Administrator's Mailbox. NOTE: Only the first six characters in the name are used in the personnel directory (Mailbox 9). | Blank
Extension Number | Enter the extension number where calls to this mailbox are to be directed. This is normally a 2- to 4-digit extension number but can be up to seven digits long. Do not use the following numbers: 0 (reserved for the operator), 9 (reserved for directory listing) or any other mailbox beginning with the number 9 (reserved for system use). This parameter can also be changed using the Administrator's Mailbox. | Blank
Passcode | A read-only field that displays the passcode for the users mailbox. |
Mailbox Type | Select a mailbox type. Extension - the mailbox type usually associated with an extension; it has the capability to record, send, and play back messages. Information - for playing informational greetings only. For example, the message (or greeting) for this mailbox could recite the company's business hours or driving directions to a company's location. This type of mailbox does not take messages. Message Only - for recording and playing back messages. It may be, but does not have to be, associated with an extension number. Message only mailboxes are for people who do not have telephones or who are frequently away from the office. Transfer Only - for playing instructions to callers to dial another number or to dial 0 to reach the company operator. This type of mailbox does not take messages. Menu Node - allow you to set up a hierarchical menu structure for multi-level auto attendant (MLAA) operation. In an MLAA system, callers reaching the Auto Attendant are routed from the main menu through to one or more additional sub menus until their call is answered. The system plays greetings for this type of mailbox and transfers callers from the mailbox to other mailboxes or extensions. Administrator - for accessing administrative functions such as recording greetings. Guest - for guests in hotels/motels with basic voice mail functionality. Front desk - for front desk staff in hotels/motels to administer guest mailboxes. This parameter can also be changed using the Administrator's Mailbox. | Extension
Prompt Language | Select a language for the voice mail prompts that the user of the mailbox hears. This parameter can also be changed using the Administrator's Mailbox. | System Default
Operator Extension (0) | Enter a location to which calls are to be directed when a caller presses"0" while listening to a greeting and recording prompt for this mailbox. A location can be any valid destination from 1 to 20 digits including extensions, external telephone numbers, hunt group access codes and system abbreviated speed dialing numbers. The default sends calls to Mailbox 0, the mailbox usually reserved for the company-wide operator. Specifying a destination other than the company-wide operator is useful in multi-tenant applications where one system services two or more businesses. With flexible Dial "0" destinations, each business can redirect calls to separate locations. This feature also accommodates users who want callers to transfer to a departmental secretary, rather than a company-wide operator. | Blank
Message Notification
Type | Select the device that the system calls to notify the mailbox user of waiting messages or select "Disable" in the Schedule field if notification is not required. The user can receive notification at any one of five locations; an extension number, an outside number, and to three different types of pagers. This parameter can also be changed using the Administrator's Mailbox. NOTE: Notification must be enabled here and in the VM Options form for notification to take place. | Extension
Number | Enter a telephone number (up to 35 digits) for the voice mail system to call for user notification. Valid digits include 0 to 9, and the [*], [#], and ['] keys. This parameter can also be changed using the Administrator's Mailbox. NOTES If there is no number in the Notification Number field, notification cannot occur even if you enable it. If two mailboxes are associated with an extension and one of those mailboxes is the operator's, when that mailbox receives a new message, it is always the operator's mailbox that is notified first. If call notification is not enabled for the operator's mailbox, no call is made to the notification number. See also Using Pagers for Message Notification. | Blank
User Access | Enable this option to allow the user to change his or her pager number. If disabled, only the system administration can change the number. This parameter can also be changed using the Administrator's Mailbox. NOTE: This option does not work for guest mailboxes. | Disabled
Schedule | Select when the system notifies the user: Around The Clock - notifies the user when the message arrives. Disabled - does not notify the user. Open Hours - notifies the user only during open business hours. Closed Hours - notifies the user only during closed business hours. | Around the Clock
Number of Messages
New | A read-only field that displays the number of new messages in the users mailbox. |
Saved | A read-only field that displays the number of saved messages in the users mailbox. |
Maximum | Enter a number up to 100 to specify the maximum number of messages that can accumulate in the mailbox. | 50
Delete Messages After | Specify how long a saved message can remain in the mailbox before it is automatically deleted: 15 Days - system default Never Delete - saved messages are never deleted Specific Number of Days - user defined value between 1 and 98 (enter the value in the Message Life field) NOTE: New messages can remain in the mailbox indefinitely | 15 days
Message Life | If you selected Specific Number of Days in the Delete Messages After field, enter a number from 1 to 98 specifying the number of days a saved message can remain in the mailbox before the system automatically deletes it. | Blank
Date/Time Stamp | Specify whether or not the system plays the date and time plus the priority and caller ID information prior to each message. If not played automatically the user can still hear the Date/Time stamp by pressing a key on the phone. | Play
Forward to Email
Forward to E-mail | Set to "Enable" to enable the Forward to Email feature. | Disabled
E-mail | The address to which the user's voice messages will be forwarded. NOTE: This Email address is not validated. If "Delete After Forward to Email" is enabled and this Email address is invalid, the voice message will be lost. | Blank
Messages Forwarded | Set to "Always" to automatically forward all incoming voice mails to the specified Email address. Set to "Manually" to let users manually forward Emails to the specified Email address. | Manually
Delete After Forwarding | Set to "Yes" to automatically delete a voice mail after it is forwarded to the specified Email address. NOTE: Delivery to the Email address cannot be guaranteed. Enabling this option can result in message loss. | No
Voice Mail Network
Local | Select if the extension is hosted on this system. | Blank
VM Server Name | Enter the name of the Voice Mail server, as defined in the VM Network Server form. | Blank
Backup VM Server Name | Enter the name of the backup Voice Mail server, as defined in the VM Network Server form. | Blank
Visual Voicemail Hunt Group | Specify the hunt group number that the Voice Mailbox belongs to. | Blank