# Programming Enterprise Gateway Trunks

The Enterprise Gateways form is used to configure the IP address and the SNMP details of the EX controller.

NOTE: This form is applicable only to the EX Controller.

## Programming the EX PRI

Fill out the forms below in the order listed.

1. Trunk Attributes form

- To check for an unused Trunk Attribute entry click Trunks > Trunk Attributes.

2. Gateway Trunk Descriptors form

3. To program click Trunks > Enterprise Gateways > Gateway Trunk Descriptors from the left navigation pane.

4. Select the required Endpoint and click Change

5. Configure the line type to T1 or E1

NOTE: If you change Line Type, the EX Controller (host) needs to be rebooted.

2. Configure Signaling to Isdn, R2, or Eam

3. Configure Endpoint Type to Te or Nt

4. Click Save.

3. Gateway Trunk Profiles form

2. To program click Trunks > Enterprise Gateways > Gateway Trunk Profiles from the left navigation pane

3. Click Add, enter the Name, enter the unused Trunk Service Number

4. Click Save

4. Gateway Trunks form

2. To program click Trunks > Enterprise Gateways > Gateway Trunks

3. Select the required endpoint and click Change.

4. Select a Trunk Profile from the drop down and click Save.

5. Gateway Configuration Scripts form

2. To program click Trunks > Enterprise Gateways > Gateway Configuration Scripts.

3. Select slot

4. Click on the drop down menu of the Default Configuration Files, to select an appropriate Mitel per slot for the PSTN circuit

5. Click Execute

6. ARS Routes

ARS continues to be provisioned in the traditional manner by assigning a route to a digit or digit string. Complete the following fields in this form:

7. Select SIP Trunk/Enterprise Gateway from the pull-down list in Routing Medium.

4. Select a Gateway Trunk Profile name from the SIP Peer Profile pull-down list.

## Programming FXO

Fill out the forms below in the order listed.

1. Trunk Attributes form

- To check for an unused Trunk Attribute entry click Trunks > Trunk Attributes.

2. Gateway Trunk Descriptors form

3. To view the status click Trunks > Gateway Trunk Descriptors > select an entry > click Change.

3. Gateway Trunk Profiles form

2. To program click Trunks > Enterprise Gateways > Gateway Trunk Profiles from the left navigation pane

3. Click Add, enter the Name, enter the unused Trunk Service Number

4. Click Save

4. Gateway Trunks form

2. To program click Trunks > Enterprise Gateways > select/change the FXO endpoint and select the Gateway Trunk Profiles name

5. Gateway Configuration Scripts form (Optional)

2. To program click Trunks > Enterprise Gateways > Gateway Configuration Scripts.

3. Select slot

4. Click on the drop down menu of the Default configuration files, to select an appropriate Mitel per slot for the PSTN circuit

5. Click Execute

6. ARS Routes

ARS continues to be provisioned in the traditional manner by assigning a route to a digit or digit string. Complete the following fields in this form:

7. Select SIP Trunk/Enterprise Gateway from the pull-down list in Routing Medium.

4. Select a Gateway Trunk Profile name from the SIP Peer Profile pull-down list.

NOTE: After successfully adding a Gateway Trunk Profile, Network Elements and SIP Peer Profile forms will have entries with the same Gateway Trunk Profiles name.