# Standalone AX Controller

The AX Controller supports

- IP phones and an IP console

- analog sets and analog trunking

- on-board digital trunking (T1, E1, and BRI based protocols are supported on MMC cards)

- connection of up to four ASUs, four ASU IIs, or any combination of up to four ASUs and ASU IIs via a Quad CIM.

If you install a 4 GB flash drive in a standalone AX Controller, it supports embedded voice mail. You manage a standalone AX Controller from its System Administration Tool.

Standalone AX Controller Configuration

Related Topics

- About the AX Controller

- Analog Media Gateway AX Controller

- Program Analog Sets and Trunks on an AX Controller

- Program Embedded T1/D4 Trunks

- Program Embedded BRI Trunks

- Program an ASU

- Program an ASU II