# LOCATE EXTENSION

## Qualifiers:

<extension number>

## Purpose:

Determines the physical location of a line for a given extension number.

## Details:

If the extension is a Hot Desk user's DN, the command will result in one of the following messages: "Hot Desk: <user's DN> Currently Not Logged in" or "Hot Desk: Login active at <registration DN>" or "Login active externally at <external number> for an External Hot Desk User. If the Hot Desk user is logged in, the command may be reissued using the registration DN.

If the extension is the prime member of a Multi-device User Group or PRG, the system response will include the following message: "This number refers to a <Multi-device User Group | Personal Ring Group>."

## Examples:

### Entry: LOCATE EXTENSION 4000

System Response:

IP Device ID: 1
Circuit Location : 1 3 1 1 1
Extension : 4000
MAC Address: 08:00:0F:00:A2:FC
Current Zone : 3

###

### Entry: LOCATE EXTENSION 26004

System Response:

The number refers to a Multi-device User Group.
Pilot Number: 26004
Members: 26004,26002,1020
IP Device ID: 14
Circuit Location : 1 3 1 14 1
Extension : 26004
MAC Address : 08:00:0F:04:DF:68
Current Zone : 3