# HSSHOWICPS

## Qualifiers:

<index_number>

## Purpose:

Displays the primary ICP(s) from which resilient device(s) have failed over.

## Details:

- To use the commands, establish a secure telnet
  Telnet or Teletype Network is an Internet standard protocol for remote terminal connection service that allows a user to interact with a system at another site as if the terminal were connected directly to the remote machine. connection to port 2002 on the primary ICP.

- Entering the command hsShowIcps without a qualifier displays all primary ICPs with associated index numbers in the range 0-99. Including an index number shows a specific primary ICP.

## Example:

### Entry: hsShowIcps 0

System Response:

Index|InUse?|Des IP Address |HealthCheck?|#OKChecks|#Devices|Devices Handoff To|#HQTicked No Reply

0| True| 10.37.159.20| True| 0| 101| 2| 0

value = 86 = 0x56 = 'V'

Where:

- InUse? means there are calls in progress

- Des IP Address means Destination IP address

- HealthCheck? means "Is health checking active for the destination ICP?" - (True/False)

- #OKChecks means Number of good health checks received

- #Devices means Number of devices to be transferred to the other ICP

- Devices Handoff To means SICP, PICP (in the case of transferring back to the primary ICP) and ICP + PICP (both)