# System Access Points

## Purpose

The System Access Points form is used to assign values to various devices in the system which require no special programming other than one parameter.

## Field Descriptions

Parameter | Description | Default Value
Night Bell Directory Number | Enter the directory number of the device or the PDN to which the night bell is connected. See Trunk Answer From Any Station (TAFAS) for more information. | Blank
DISA Forced Account Code - Directory Number | Enter the directory number by which the DISA trunk using the forced account code feature is to be identified in the Trunk Attributes form. | Blank
DISA Directory Number | Enter the directory number by which the DISA trunk is to be identified in the Trunk Attributes form. | Blank
Music Source | If you are not using the system Music on Hold (MoH), select "None". If using embedded MoH, select "Embedded". For analog or digital MoH, select "External". For MoH over IP, select "IP Endpoint". Selecting "External" requires an entry in the Music Source Port - Location ID field. If left blank, your selection for Music Source will not be saved. NOTE: Changing the music source terminates background music currently playing at stations. Music does not automatically resume with the selection of a new source; users must turn it back on using the Music feature key or via the Superkey (if supported). To avoid inconveniencing users, make changes during off-hours when possible. | None
Music Source Port - Location ID | Enter the physical location identification (PLID) of the circuit to which the external Music on Hold circuit is connected. Not applicable when "Music Source" is set to "None" or "Embedded". | Blank
Music Source - Directory Number | Enter a local SIP or IP DN (0 to 9 digits, * and # characters only). NOTE: This field is enabled when you select "IP Endpoint" in the Music Source field. Data in this field is not shared. | None
Message Center - Directory Number | This field is not applicable to MiVoice Business. Leave blank. | Blank
Milliwatt Test Directory Number | Enter the directory number used to access the milliwatt test for the Line Measure Tool. | Blank
Balance Test Directory Number | Enter the directory number used to access the balance test. This field is associated with the Line Measure Tool. It should be used only by Mitel Product Support. | Blank
100 Test Directory Number | Enter the directory number used to access the 100 test. This field is associated with the Line Measure Tool. It should be used only by Mitel Product Support. | Blank
MNMS: Event Indication Number | This field is not applicable to MiVoice Business. Leave blank. | Blank
MNMS: Event Indication Routing Number | This field is not applicable to MiVoice Business. Leave blank. | Blank
Administrative Directory Number | Enter the directory number to which the BRI NSU will send DPNSS date and time requests. This same number is also entered in the BRI programming "PBX maintenance address". | Blank
Voice Dial Access Number | Enter the directory number of the Mitel Speech Server system (or NuPoint/MiCollab Nupoint UM equivalent). The digit string must translate into a valid hunt group, extension number, remote directory number, or speed dial to ARS. | Blank
Hot Desking Access Number | Enter the DN that terminates the DID number dialed by external hot desking users to access system resources, including extensions, voice mail, outgoing trunks etc. | Blank
Hot Desking Callback After Digit Collection Number | As above but for Blackberry® users and users of other devices that support "smart dialing." With smart dialing, users can store the Callback DID number to the device for quick dialing. This number can be any valid extension, hunt group, ACD path, or ARS destination. | Blank
Hot Desking Callback Before Digit Collection Number | Enter the DN that terminates the DID number dialed by external hot desking users to request a Callback. | Blank
Meet Me Conference Access Number | Enter the Meet Me Conference access number. This is the number that users dial to access Me Meet Conference. | Blank