# SIP DNS SHOW

## Qualifiers:

None.

## Purpose:

Displays the mappings used by SIP NAPTR, SRV, A/AAAA records.

## Details:

For a SIP NAPTR query, the system displays NAPTR records, SRV and A/AAAA records found and used to resolve the address. Also, indicates whether the record is invalidated.

For a SVR query, the system displays the query type and associated A/AAAA records.

For a A/AAAA query, the system displays the order of the list of addresses.

## Example:

### Entry: SIP DNS SHOW

### System Response:

pinehill.myco.com

NAPTR Query

sip: protocol=Undefined port=0 [ client=Event InUse=0 #ip=4 udp]

Created= Tue Oct 17 11:58:12 2017 LastUsed=Tue Oct 17 11:58:44 2017

Results:

NAPTR index=1 order=10 pref=100 flag=S service=SIP+D2T scheme=sip:

replacement=_sip._tcp.pinehill.myco.com

NAPTR index=2 order=20 pref=100 flag=S service=SIP+D2U scheme=sip:

replacement=_sip._udp. pinehill.myco.com

SRV index=1 key=_sip._tcp. pinehill.myco.com naptr[10 100] priority=1 weight=5 port=5060

target= pinehill.myco.com

A/AAAA

10.32.10.127

2003:34:12:10::127

SRV index=2 key=_sip._udp. pinehill.myco.com naptr[20 100] priority=1 weight=5 port=5060

target= pinehill.myco.com

A/AAAA

10.32.10.127

2003:34:12:10::127

steeplechase.myco.com

SRV_UDP Query

sip: protocol=Udp port=0 InUse=0 #ip=2 udp

Created= Tue Oct 17 12:30:57 2017 LastUsed=Tue Oct 17 12:31:30 2017

Results:

SRV index=1 key=_sip._udp.steeplechase.myco.com naptr[-1 -1] prior[1 5] port=5060

target= steeplechase.myco.com

A/AAAA

10.43.16.17

2003:34:12:16::17