# HSHANDBACK

## Qualifiers:

None

## Purpose:

Cancels the hsHandoff command.

The hsHandoff command is equivalent to the HST Courtesy Handoff maintenance command in the System Administration Tool.

After you enter this command,

- any resilient devices that have NOT already been handed off to the secondary ICP will remain on the primary.

- any resilient sets that have already been handed off to the secondary ICP are sent back. This is not instantaneous, but all the devices will be sent back over time without interrupting calls in progress.

## Details:

- To use the commands, establish a secure telnet
  Telnet or Teletype Network is an Internet standard protocol for remote terminal connection service that allows a user to interact with a system at another site as if the terminal were connected directly to the remote machine. connection to port 2002 on the primary ICP.

- You must enter this command on the primary ICP.

- As the handback is being completed, the primary ICP will respond to health checks sent by the secondary.

## Example:

### Entry: hsHandback

System Response:

Safely handback IP Devices to their primary-ICP.

Please wait ...

value = 0 = 0x0

->