# Resilient T1/E1 Framers

## Purpose

The Resilient T1/E1 Framers form is used to program the unit to which each module connects, and to select the interface type for each port.

Use this form when performing the following tasks:

- Program Embedded PRI/QSIG

- Program Embedded T1/D4 Trunks

## Field Descriptions

Parameter | Description | Default Value
T1/E1 Framers
Controller Module | System-generated, protected field. Indicates the module's position in the controller. |
Unit | Enter a unit number from interfaces 2 - 16. | Blank
Comment | Enter any applicable comments (optional). | Blank
T1/E1 Framer Port Configuration
Port | System-generated, protected field. Displays the port number for each module. |
Interface Type | Select an interface type: For embedded T1/D4, select "T1" For embedded PRI/QSIG, select "T1" or "E1" For embedded DPNSS/DASS II, select "T1" or "E1" | Blank