# ALARMS

## Qualifiers:

None

## Purpose:

Displays circuit fault information for all alarm categories.

## Details:

See alarm categories for a description of the alarms and SHOW FAULTS for details about the faults that are responsible for them.

If digital links show ALARMs, but links are not at fault, check DTSTAT for the specific link. If there are DTSTAT errors, use DTSTAT clear to eliminate the alarm.

## Example:

### Entry: ALARMS

System Response:

Current System Alarm: MAJOR viewed from Active

Category | Total in System | Unavailable | Alarm Threshold Percentage
Total | % | Alarm | MINOR | MAJOR | CRITICAL
Lines | 160 | 16 | 10% | Minor | >0% | 20% | 100%
Trunks | 140 | 79 | 56% | Major | >0% | 10% | 100%
Receivers | 16 | 0 | 0% |  | >0% | 25% | 100%
Inact. receivers | 12 | 0 | 0% |  | >0% |  |

NOTE: The complete system response is not shown in the above example.