# Bandwidth Management

## Purpose

The Bandwidth Management form is used to set the parameters to manage bandwidth on MiVoice Business and to enable the Bandwidth Management feature.

Use this form when performing the following tasks:

- Program Bandwidth Management

- Model Network Connectivity

- Display Bandwidth Historical 15 Minute

- Set Bandwidth Alarm Thresholds

For more information:

- Bandwidth Management - Introduction

- Using Bandwidth Statistics

## Conditions

None

## Field Descriptions

Parameter | Description | Default Value
Call Admission Control Enabled | Select the check box to enable the bandwidth management call admission control feature. Clear the check box to disable this feature. | No
Bandwidth Reporting & Statistics |
Bandwidth Management Statistics and Reporting Enabled | Select the check box to enable bandwidth reporting and statistics. Clear the check box to disable this feature. | No
Rising Threshold for Bandwidth Alarm (%) | Enter a percentage for the rising threshold. This threshold triggers an alarm whenever the bandwidth in use exceeds the rising threshold value at a zone access point (ZAP) managed by the ICP. | Blank
Falling Threshold for Bandwidth Alarm (%) | Enter a percentage for the falling threshold. MiVoice Business clears the alarm whenever the bandwidth in use falls below the threshold value at the ZAP. | Blank