# ANI/DNIS/ISDN Number Delivery - Programming

## Conditions and Feature Interactions

- Only T1/D4 DID or T1/D4 E&M trunks that are programmed with a digital DID or digital E&M trunk circuit descriptor can receive ANI and DNIS digits. The trunk must use DTMF signaling and have a wink timer.

- The Class of Service of the trunk controls the ANI/DNIS display.

## Programming

To program a trunk to receive ANI/DNIS numbers:

- Class of Service Options form

- enable ANI/DNIS/ISDN Number Delivery Trunk in the trunk's Class of Service.

- For DID trunks, enable Display DNIS/Called Number Before Digit Modification in the trunk's Class of Service (if desired).

To display ANI/DNIS information on display telephones and consoles:

- Class of Service Options form

- enable Display ANI/DNIS/ISDN Calling/Called Number.

- enable the following options as required:

- - To display the ANI/ISDN calling number only, enable Display ANI/ISDN Calling Number Only.

  - To display unmodified DNIS numbers, enable Display DNIS/Called Number Before Digit Modification.

  - To display ANI, DNIS, and trunk information related to a station's keyline or multicall line (not the station's prime line), enable Display Caller ID on Multicall/ Keylines.

To program the system to include the ANI and DNIS digits in the SMDR records:

- SMDR Options form

- Enable ANI/DNIS/ISDN/CLASS Number Delivery Reporting.

NOTE: See Station Message Detail Recording for a summary of the SMDR report format.

## Device Support

Not applicable

## Operation

None

Related Topics

- ANI/DNIS/ISDN Number Delivery Description

- ANI/DNIS/ISDN Number Delivery Conditions