# E2T Comms Alarm

## System/Sub-System

MiVoice Business: Hardware

## Description

The alarm is raised if the hardware is detected and the E2T card does not respond.

NOTE: E2T Comms alarm is applicable to MXe Expanded Controller.

## Alarm Status

The major threshold is > 0.

#### Possible Cause | #### Corrective Action
--- | ---
Configuration issue of E2T card. Hardware failure of E2T card. | Refer to Technician’s Handbook and check bootline configuration of E2T card. Replace E2T card.