# Wireless IP Sets

## Purpose

The Wireless IP Sets form is used to program Symbol IP devices, SpectraLink Wireless Telephones, and Mitel IP-DECT OpenPhones on the MiVoice Business system. To display the next page of entries, click Next. To display the first page of entries again, click Data Refresh.

Use this form when performing the following tasks:

- Program a Symbol NetVision Phone

- Program SpectraLink Wireless Telephones

- IP-DECT Wireless Solution

## Conditions

- When deleting IP sets, you must also delete the corresponding directory entries and voice mailboxes.

## Field Descriptions

Parameter | Description | Default Value
Device ID | System-generated, protected field. Identifies the IP telephone. NOTE: The form will only display the number of IP devices that have been purchased (up to a maximum of 700 IP devices). You can only program the purchased number of IP telephones. |
Device Type | Select the required device type. | Netvision IP
Directory Number | Enter a unique internal directory number up to seven digits in length assigned to the line circuit. | Blank
Local-only DN | Allows you to specify the directory number as a local-only directory number in a cluster. | Not Selected
Wireless PIN | Enter a 4 digit PIN number (used for NetVision only). | Blank
ACD Enabled | Select "Yes" if the telephone is to be an ACD set. NOTE: This field cannot be changed from "Yes" to "No" if the telephone is part of an ACD hunt group. | No
Line Type | System-generated, protected field. Contains a default value of "not assigned". Once the line is programmed, the field shows "single line". Once a group is created, the field shows either "key system" or "multicall" as appropriate. |
Interconnect Number | Enter a number between 1 and 64 that references an entry in the Interconnect Restriction form. | Blank
Language | System-generated, protected field. Indicates the set operating language. NOTE: Only English is supported for Symbol wireless phones. |
MAC Address | Enter the MAC address of the device (if required). IP-DECT OpenPhones: You do not need to enter the MAC addresses of the OpenPhones if the OpenPhones have the latest version of firmware installed. Ensure that you download and install the latest OpenPhone firmware. Refer to the IP-DECT Technical Manual for instructions. SpectraLink Wireless Telephones: You do not need to enter the MAC Address of the SpectraLink wireless phone. | Blank
Tenant Number | Enter the number of the set's tenant. | 1 (landlord)
User PIN | Enter a password for the User PIN. The PIN can only include digits from 0 to 9 and can be from 0 to 10 digits in length. | Blank
Confirm User PIN | Re-enter the password to confirm. | Blank
Service Level | System-generated, protected field. Identifies the Service Level assigned in the User and Services Configuration form NOTE: All devices added on this form have Full Service This Service Level indicates that the directory number (DN) is assigned to a standard user and device with full telephony functionality.. Use the User and Services Configuration form to program other Service Levels. |