# BSSID to CESID Mapping

## Purpose

The BSSID to CESID Mapping form allows you to map CESIDs to on-premise WAPs. This form only needs to be configured for 5624/5634 wireless devices.

NOTE: The form is empty by default and there are no limits on number of entries.

## Field Descriptions

Parameter | Description | Default Value
BSSID | Enter the BSSID. Alphanumeric characters allowed are - 0-9, a-f and A-F. Ensure to include the proper colons. For example: a1:b2:c3:d4:ef:f6. NOTE: The field accepts a MAC address format that corresponds to the BSSID on the WAP. | Blank
CESID | Enter the CESID. 0-9 are allowed with maximum 12 digits. | Blank
BSSID Label | Enter the comment with the location of the access point. This is a comment field with 21 alpha numeric support | Blank