# HSHELP

## Qualifiers:

### None

## Purpose:

Displays a list of the HandoffService commands with a brief description of their function.

## Details:

To use the commands, establish a secure telnet
Telnet or Teletype Network is an Internet standard protocol for remote terminal connection service that allows a user to interact with a system at another site as if the terminal were connected directly to the remote machine. connection to port 2002 on the primary ICP.

## Example:

### Entry: hsHelp

System Response:

---------------------------------------------------------------------------------

HandoffService Commands Descriptions

---------------------------------------------------------------------------------

hsShowIcps show a list of handoff ICPs

hsShowIcp index show a given ICP

hsShowSets show all resilient devices

hsShowSet index show a given device

hsHandoff issued at 1st-ICP: managed-failover to 2nd-ICP

hsHandback issued at 1st-ICP: cancel/reverse the above

hsPushback issued at 2nd-ICP: forced-failback to 1st-ICP

.

.

.

hsDebug 1/0 on/off more system logs

hsTrace 1/0 on/off handoff process trace on console

---------------------------------------------------------------------------------

value = 83 = 0x53 = 'S'

Where:

- 1st-ICP means primary ICP

- 2nd-ICP means secondary ICP