# EDT HELP

## Qualifiers:

None

## Purpose:

Displays the maintenance commands that are provided for embedded digital trunks (PRI, BRI, QSIG, and T1/D4).

## Example:

### Entry: EDT HELP

System Response:

2005-03-11 11:36:09

All commands begin with EDT followed by either < HELP, SHOW, TRACE, ENABLE, DISABLE, DELETE >

Terminate the following commands with either <ALL, BRI, PRI, T1D4>
SHOW FRAMER STATS - display framers statistic
SHOW FRAMER CONFIG - display framers configuration
SHOW FRAMER REGS - display framers registers
SHOW LINK CONFIG - display link configuration
SHOW LINK STATUS - link status

Terminate the following commands with <CABINET> <SHELF> <SLOT> <PORT>
SHOW VDSU ALARMS - display alarms
SHOW VDSU STATS - display statistic
SHOW VDSU CHANNELS - display channels

2005-03-11 11:36:09
The following message trace commands are terminated with <CABINET> <SHELF> <SLOT> <PORT>

TRACE TSP L2L3 - toggle SP Stack layer 2/3 CC verbose msg trace
TRACE TSP CC - toggle SP Call Control verbose msg trace
TRACE TSP MTCE - toggle SP Maintenance verbose msg trace
TRACE TSP SRVC - toggle SP Service verbose msg trace
TRACE VDSU UAPI - toggle UAPI message tracing
TRACE VDSU VB - toggle Verbose messaging
TRACE VDSU CP - toggle Call Processing message tracing
TRACE VDSU NAMNUM - toggle Name Number message tracing
ENABLE LOGTOFILE - start logging traces to file on the hard drive
DISABLE LOGTOFILE - stops logging the traces to a file on the hard drive

2005-03-11 11:36:09
ENABLE DBFLAGS - obtain ALL debug flag settings stored on the hard drive
DISABLE DBFLAGS - set all debug flags to default setting i.e. false
DELETE DBFILES - delete the contents of ALL debug files, default system startup

2005-03-11 11:36:09

The following commands do not require any additional arguments
SHOW VDSU TABLE - list all the VDSUs on the system
SHOW LINK INFO - link information, i.e. digital trunking type