# Dual T1/E1 Framers

## Purpose

The Dual T1/E1 Framers form is used to program the two configurable hybrid ports on each Dual T1/E1 Framer. Each hybrid port can be programmed for an embedded PRI, DNPSS, or T1D4 trunk.

Use this form when performing the following tasks:

- Program Embedded PRI/QSIG

- Program Embedded T1/D4 Trunks

## Conditions

- This form does not apply to the CX II and CXi II controllers.

## Field Descriptions

Parameter | Description | Default Value
Dual T1/E1 Framers
Controller Module | System-generated, protected field. Indicates the module's position in the controller. |
Unit | Enter a unit number from interfaces 2 - 16. Two ports can be configured on each dual framer. | Blank
Comment | Enter a name (up to 30 characters) to describe the framer port. | Blank
Dual T1/E1 Framer Port Configuration |
Port | System-generated, protected field. Displays the port number for each module. |
Interface Type | Select an interface type from the drop-down list: For embedded T1/D4, select "T1" For embedded PRI/QSIG, select "T1" or "E1" For embedded DPNSS/DASS II, select "T1" or "E1" | Blank