# BLF REFRESH

## Qualifiers:

CEID <CEID index>

CEID ALL

## Purpose:

Refreshes remote busy lamps after work on inter-system trunks.

## Details:

The command functions from a broadcasting system perspective.

Both variants of the command refresh only remote busy lamps monitoring devices that are local to the invoking system.

The command BLF REFRESH CEID ALL will refresh all remote busy lamps.

The command BLF REFRESH CEID <CEID INDEX> will refresh the busy lamps on the clustered system specified by the three-digit Cluster Element Identifier (CEID) Index number.

## Examples:

### Entry: BLF REFRESH CEID 1

System Response:

Commence BLF refresh for CEID 001.
BLF refresh complete for CEID 001.

### Entry: BLF REFRESH CEID 2

System Response:

BLF REFRESH of local busy lamps not available.

### Entry: BLF REFRESH CEID ALL

System Response:

Commence BLF refresh for CEID 001.
BLF refresh complete for CEID 001.
Commence BLF refresh for CEID 002.
BLF REFRESH of local busy lamps not available.
Commence BLF refresh for CEID 003.
BLF refresh complete for CEID 003.
BLF refresh complete for all CEIDs.