# Programming Controller Modules

## Before You Begin

Ensure that the Quad CIM, Dual T1/E1 Framer, T1/E1 Framer, or Quad BRI Framer is installed as shown in the Technician's Handbook.

## Programming

To program a controller module:

1. Controller Module Configuration form

Select one of the following from the "Programmed Type" field:

2. "Quad CIM" for a Quad CIM module

3. "Dual Framer" for a Dual T1/E1 Framer (Proceed to step 2)

4. "T1/E1 Combo" for a T1/E1 Framer (Proceed to step 2)

5. "Quad BRI" for a Quad BRI module (Proceed to step 3)

2. Dual T1/E1 Framers form ( ) or Resilient T1/E1 Framers form ( )

Click Change and assign a Unit number (2 - 16) and an optional 30-character comment.
Click Change Member and assign the interface type (T1 or E1) for each port on the module.

2. For embedded T1/D4, select "T1"

3. For embedded PRI or QSIG, select "T1" or "E1" as required

4. For embedded DPNSS/DASS II, select "T1" or "E1" as required

3. Quad BRI Framers form

Click Change and assign a Unit number (2 - 16) and an optional 30-character comment.

By default, the BRI interface type is assigned to each port on the module.

NOTES

- If you program the second T1 or E1 port at a later time, any calls established on port 1 will be disconnected when you configure port 2. Manbusy the first port before you begin to program the second port.

- For procedures on programming embedded digital links, see

- T1/D4 (feature details).

- Program Embedded PRI/QSIG Trunks (feature details)

- Program Embedded BRI Trunks (feature details)