# Privacy Release

## Description

Allows members of a Key System Group to disable automatic call privacy protection to allow another member of the group to join the call. When a new member enters the call the original members receive a conference tone and the privacy feature is restored.

## Conditions and Feature Interactions

- Prior to activating the feature the set must be in the talking state.

- The feature can only be selected when the line being used is a member of a key system group.

- Privacy Release does not apply if a station that has "Conference" and "Privacy Released" in its Class of Service is included in the call, unless that station user has activated the Call Privacy feature.

- The feature cannot be selected when:

- any user in the call has another call on consultation hold,

- one of the parties in the call is an attendant or a non-busy extension,

- the set is in display, select features or add held mode,

- all members of the key system group are involved in the call,

- the set is involved in a conference that has been placed on hold,

- the set is involved in a conference having the maximum number of members.

- This feature is not applicable to the Mitel 5001 IP Phone, Mitel 5201 IP Phone or Symbol Wireless Phones.

- When a conference is established with the privacy release feature, the parties do not hear a conference tone if they all have Disable Conference Join Tone set to "Yes" in their COS.

- Key system group members participating in a conference in which the Privacy Release feature has been invoked lose Trans/Conf key functionality (including soft hold) for the duration the conference.

## Programming

1. Class of Service Options ( ) or User and Services Configuration form

- Enable the "Conference" option.

2. Multiline Set Keys form

- To provide feature key activation of privacy release for the following sets program a PRIVACY RELEASE (LINE PRIVACY) feature key or use Superkey (see Feature Keys for more information on Superkey programming):

5005 IP Phone, 5205 IP Phone, 5207 IP Phone, 5010 IP Phone, 5212 IP Phone, 5215 IP Phone, 5215 IP Phone (Dual Mode), 5020 IP Phone, 5220 IP Phone, 5220 IP Phone (Dual Mode), 5224 IP Phone, 5312 IP Phone, 5324 IP Phone, Navigator, TeleMatrix 3000IP Phone, and 69xx IP Phones.

5020 IP Phone, 5220 IP Phone and 5220 IP Phone (Dual Mode) telephone users can program a LINE PRIVACY feature key from their set.

## Device Support

- Supported on all devices.

## Operation

When a station which has "Conference" and "Privacy Released" set in its Class of Service is included in a call, any other member of that group can enter the call by pressing the appropriate line key or lifting the handset (station).

When a station has activated the call privacy feature, or is not included in the call, and has "Conference" set in its Class of Service, privacy can be released in the following manner:

#### 5005 IP Phone, 5010 IP Phone, 5020 IP Phone, 5140 IP Phone, 5205 IP Phone, 5207 IP Phone, 5212 IP Phone, 5215 IP Phone, 5215 IP Phone (Dual Mode), 5220 IP Phone and 5220 IP Phone (Dual Mode), 5224 IP Phone, 5240 IP Phone; 5312 IP Phone, 5320/5320e IP Phone, 5324 IP Phone, 5330/5330e IP Phone, 5340/5340e IP Phone; 5360 IP Phone, Navigator, TeleMatrix 3000IP Phone, 5560 IPT, and 69xx IP Phones

To turn privacy on:

- Press the Rel Privacy softkey, the Privacy release feature access key, or navigate to the Line Privacy option under the Superkey menu.

To turn privacy off:

- Press the Make Private softkey, the Privacy release feature access key, or navigate to the Line Privacy option under the Superkey menu.

NOTE: The "Privacy Release" COS option must be disabled for the station using this method of privacy release.

Related Topics

- Feature Keys

- Groups - Key System and Multicall