# Personal Speed Call Allocation

## Purpose

The Personal Speed Call Allocation form is used to allocate resources, on a per-directory number basis, to permit the definition and storage of personal speed calls. It is used to allocate a quantity of personal speed call numbers to ONS lines, Mitel display telephones, and attendant console prime directory numbers.

Use this form when performing the following tasks:

- Speed Call - Personal

## Conditions

- A Multi-Device
  This Service Level indicates that the directory number (DN) is assigned to a user that has only basic telephony functionality (e.g., emergency or attendant calls) until programmed as a member of a Multi-Device user group or suite. The DN does not use an IP User License. However, the group or suite has a Multi-device Users or Multi-device Suites license which one person can use at a time in order to receive full telephony service. DN can be programmed as an allocated resource, provided that the DN is the prime member of a Multi-device User Group.

## Field Descriptions

Parameter | Description | Default Value
Directory Number | System-generated, protected field. Lists all ONS, Mitel telephones, and attendant console directory numbers that are currently assigned in the system. The directory numbers are listed in lexicographical order. |
Name | System-generated, protected field. Contains the name associated with the directory number in the Telephone Directory form. |
Entries Allocated | Enter the number of speed call numbers allocated, in multiples of 10. Personal speed call numbers are assigned in multiples of 10 up to a limit of 100. If the Entries Allocated entry is blank for a given directory number, the system assumes that no entries are to be allocated to the directory number. | Blank
Entries Used | System-generated, protected field. Shows how many speed call numbers are currently in use for the given directory number. |