# HSTRACE

## Qualifiers:

1 or 0

## Purpose:

Enables or disables monitoring of events associated with the handoff operations (hsHandoff. hsHandback, hsPushback) on the telnet console screen.

## Details:

- To use the commands, establish a secure telnet
  Telnet or Teletype Network is an Internet standard protocol for remote terminal connection service that allows a user to interact with a system at another site as if the terminal were connected directly to the remote machine. connection to port 2002 on the primary ICP.

- Tracing is automatically disabled after each hand off operation completes.

## Example:

### Entry: hsTrace 1

System Response:

System Response:

-> hsTrace 1

value = 1 = 0x1

-> hsHandoff

Safely handoff IP Devices to their Secondary-ICP, please wait ...

To cancel/recover this action, use hsHandback command.

value = 0 = 0x0

->

->

HS recv HANDOFF_QUERY_REPLY: DestIpAddr = 10.37.106.20, RespIpAddr = 10.37.159.20, NumSetsToHandoff = 27

HS sent HANDOFF_QUERY: DestIpAddr = 10.37.159.20, OrigIpAddr = 10.37.106.20, NumSetsToHandoff = 392

HS recv HANDOFF_QUERY_REPLY: DestIpAddr = 10.37.106.20, RespIpAddr = 10.37.159.20, NumSetsToHandoff = 5

HS sent HANDOFF_QUERY: DestIpAddr = 10.37.159.20, OrigIpAddr = 10.37.106.20, NumSetsToHandoff = 387

.

.

.

hsTrace 0

value = 0 = 0x0

->