# Call Forwarding Profile

## Purpose

Use this form to set up Call Forwarding or to change or delete the Call Forwarding currently in effect at one or more extensions.

Deleting Call Forwarding turns it off and removes the destination number. Each deletion applies to only one Call Forwarding type at a time. So if an extension has multiple Call Forwarding types—for example, Busy Internal and No Answer External—two Delete operations are required to completely disable Call Forwarding.

NOTE: If a Directory Number (DN) is member of a MdUG, then DNs of only prime members are displayed in this form.

## Field Descriptions

Parameter | Description | Default Value
Number | Select the directory number of the extension to change its Call Forwarding setup. To change multiple contiguous extensions, select the first directory number in the range. Then, click Add, Change, or Delete. |
Call Forward Type | Select the Call Forward type: Always, Busy Internal, Busy External, No Answer Internal, No Answer External. This field is ready-only for Change operations. |
Forwarding Destination | Enter the destination number where calls to this extension will be forwarded. See the Call Forward feature description for valid destinations. | Blank
Forwarding Enabled | Select On or Off to enable or disable the selected Call Forwarding type. NOTE: This option only applies to the prime lines of multi-line sets, including SIP devices. To disable a Call Forwarding Profile entry for any other type of directory number, such as analog phones, hunt groups, ring groups and non-prime lines, the entry must be deleted. | Off