# Call Rerouting Always Alternatives

## Purpose

The Call Rerouting Always Alternatives form is used to specify routing information for calls routed to the "always alternative" numbers. The rerouting information is defined based on the originating device (DID trunk, TIE trunk, CO trunk or internal call).

Use this form for the following tasks:

- Programming Call Rerouting

- Program Auto Attendant

- Program Night Service - Automatic

## Field Descriptions

Parameter | Description | Default Value
Always Alternative Number | System-generated, protected field. An index value identifying an Always Alternative Number entry in the range 1 to 175. The range can be higher in the Dimension Section form. See Flexible Dimensioning for more information. |
Originating Device DID | Select "Reroute" to reroute the DID calls to the directory number specified in the last column of the form. Select "No Reroute" to permit the call to be completed. | No Reroute
Originating Device TIE | Select "Reroute" to reroute the TIE trunk calls to the directory number specified in the last column of the form. Select "No Reroute" to permit the call to be completed. | No Reroute
Originating Device CO | Select "Reroute" to reroute the CO turnk calls to the directory number specified in the last column of the form. Select "No Reroute" to permit the call to be completed. | No Reroute
Originating Device INT | Select "Reroute" to reroute the internal calls to the directory number specified in the last column of the form. Select "No Reroute" to permit the call to be completed. | No Reroute
Directory Number | Enter the directory number to which the call is to be routed. The directory number field must be blank if all of the originating device fields (DID trunk, TIE trunk, CO trunk, or internal call) are set to "no reroute". The Directory Number rerouted must be one of the following: the directory number of a station the directory number of a "Single Line" type key on a multi-line set the directory number of a key system, multi-call, or mixed multi-line appearance group a hunt group pilot number a ring group pilot number a personal ring group pilot number attendant console group directory number a system speed call number. | Blank
Comment | (Optional) Enter a comment (a maximum of 26 ASCII characters) on the entry. | Blank