# SHOW EX CONFIGURATION HELP

## Qualifiers:

None

## Purpose:

Displays help text for the supported, configurable EX parameters.

## Details:

This command displays the following details about the supported, configurable EX parameters:

1. Parameter Name

2. Help text for the parameters (for example, range of supported values)

## Example:

### Entry: SHOW EX CONFIGURATION HELP

### System Response:

AllowedDTMFMap.01 -> is text

AllowedDTMFMap.02 -> is text

AllowedDTMFMap.03 -> is text

AllowedDTMFMap.04 -> is text

AllowedDTMFMap.05 -> is text

AllowedDTMFMap.06 -> is text

AllowedDTMFMap.07 -> is text

AllowedDTMFMap.08 -> is text

AllowedDTMFMap.09 -> is text

AllowedDTMFMap.10 -> is text

MaximumFacilityWaitingDelay.Slot1/E1T1 -> has a range of 0 to 1500 milliseconds

Pots.FxoDialToneDetectionMode -> is an enum list of 100-Disable,200-CountryTone

Pots.FxoDialToneDetectionTimeout -> has a range of 1300 to 10000 milliseconds

Pots.FxoPreDialDelay -> has a range of 0 to 1000 milliseconds

Pots.FxsDefaultVisualMessageWaitingIndicatorType -> is an enum list of 100-Fsk,200-FskAndVoltage

To set any of the above values, use 'SET EX CONFIGURATION parameter value".

Related Topics

- SHOW EX CONFIGURATION

- SET EX CONFIGURATION