# Tone Demonstration

## Description

Tone Demonstration allows you to hear the tones provided on the system.

## Conditions and Feature Interactions

- Dialing any string of digits (other than the specified two-digit identification code) results in either termination of the Tone Demonstration or return of random tones.

- During Tone Demonstration, if you flash the switchhook, you will hear Transfer dial tone, and you will exit Tone Demonstration.

- If you do not enter an identification code within 30 seconds, you will exit Tone Demonstration.

- If you select waiting tone (23), you will hear either music (if provided) or silence.

- Not supported on SIP devices.

## Programming

- Feature Access Codes form

- Assign a feature access code to Tone Demonstration.

## Device Support

- Supported on all devices.

## Operation

#### All telephones

To use Tone Demonstration:

1. Lift the handset.

2. Dial the Tone Demonstration feature access code.

3. Dial the tone identification code from the table below.

4. Do one of the following:

5. To exit, hang up.

6. To listen to another tone, dial another tone identification code

Tone Identification Code | Tone
10 | silence
11 | dial tone
12 | transfer dial tone
13 | busy tone
14 | do not disturb tone (special busy tone)
15 | standard ringback tone
16 | special ringback tone
17 | reorder tone
18 | conference tone
19 | camp-on tone
20 | override tone
21 | interrupted dial tone
22 | interrupted dial tone with message waiting tone
23 | waiting tone
24 | paging tone
25 | dial tone with message waiting tone
26 | data connect tone
27 | extended second dial tone
28 | feature active tone
29 | confirmation tone
30 | congestion tone
31 | Channel Associated Signaling ( CAS) tone
33 | ringer pitch adjust tone