# ISDN Outgoing Numbers

## Purpose

This form allows you to select the outgoing numbering plans for Euro ISDN Standard trunk variants provided by the embedded PRI/ BRI functionality available on the 3300 ICP controller. To meet the specific ISDN requirements of a European region, you can select the Calling Number and Called Number parameters.

Use this form when performing the following tasks:

- Program Embedded BRI Trunks

- Program Embedded PRI/QSIG Trunks

- ISDN Protocol

### Calling Number

For the calling number, you can set the Type of Number and Numbering Plan ID. When a Party Number Information Element is included in the outgoing SETUP message, this feature takes effect and the Type of Number and Numbering Plan Fields of the Calling Party Number will be set to the values programmed in this form.

### Called Number

For the called number, you can set the Numbering Plan ID. This setting applies to outbound calls only. When a Called Party Number Information Element is included in the outgoing SETUP and INFO message, this feature will take effect and the Numbering Plan ID will be set to the value programmed in this form.

## Conditions

- This feature only applies to BRI or E1 interfaces running the Euro Standard protocol of the Euro ISDN variant.

## Field Descriptions

Parameter | Description | Default Value
Controller Module | System-generated, protected field. Identifies the module position (1-4) in the controller. |
Port | System-generated, protected field. Identifies the port (1 or 2) in the module. |
Calling Number
Type of Number | Set the Type of Number field to Unknown, International Number, National Number, Network Specific, or Subscriber. | Unknown
Numbering Plan ID | Set the Numbering Plan ID to Unknown, ISDN/Telephony, Data, Telex, National Standard, or Private. | ISDN/Telephony
Called Number
Numbering Plan ID | Set the Called Number - Number Plan ID to Unknown, ISDN/Telephony, Data, Telex, National Standard, or Private. | Unknown

## Selecting the Outgoing Numbering Plans

1. From the Selection menu, select View by Category.

2. Select Trunks > Digital > Digital Trunks.

3. Depending on trunk type, select

4. ISDN-BRI or

5. ISDN-PRI and then click E1.

4. Click Outgoing Call Characteristics and then click ISDN Outgoing Numbers.

   NOTE: The form only shows the links that are either PRI/E1 Euro ISDN/ Euro Standard or BRI-T interfaces.

   CAUTION: If you change the protocol variant in the ISDN Protocol form, the programming detail in this form will be deleted.

5. Select the Controller Module/Port of the trunk and click Change (or Change All).

6. Select the

7. Type of number

8. Calling Number Number Plan ID

9. Called Number Numbering Plan ID

7. Click Save.