# QSIG Calling Name

QSIG Calling Name allows the system to send and receive the name of the caller; in turn, the called party will see the name of the caller on the telephone display screen if the appropriate Class of Service options are set. QSIG supports the Calling Name Presentation and Restriction option

NOTE: QSIG Calling Name currently supports a maximum of 15 characters.

Related Topics

- QSIG Description

- QSIG Conditions

- QSIG Operation

- QSIG Programming