# Configuring Bandwidth Management for Hot Desking

You can track the bandwidth utilization of Hot Desk users if the ICP manages both ZAPs on the voice media path between the devices that the hot desk user logs into.

BWM for Hot Desking

In the example above, ICP A manages both ZAP 1 and ZAP 2. Because ICP A has visibility of both ZAPs, bandwidth utilization tracking and management is possible.

You would program the configuration above in the following way:

Network Elements |  | Zone Tree Assignment
Name | Zone |  | Zone | Parent Zone | Perimeter
Chicago ICP A (Local) | 4 |  | 4 | 3 | No
Detroit ICP B | 2 |  | 2 | 3 | No
|  |  | 3 |  | No

Zone Access Point Assignment (Summary)
Zone | Zone Access Point ID | Zone Access Point Label | Bandwidth Limit | Network Element
2 | 1 | Detroit-Chicago (1) | 500 | ICP A
2 | 2 | Detroit-Chicago (2) | 500 | ICP B

Related Topics

- Program Bandwidth Management