# L2 STATUS SWITCH

## Qualifiers:

None

## Purpose:

NOTE: This maintenance command is not applicable to server-based MiVoice Business for Industry Standard Server, MiVoice Business Virtual MiVoice Business platforms.

Provides general Layer 2 (L2) switch information. For more detailed information, use the L2 Stat Port command.

## Details:

Field Name | Description
L2 Switch uptime | The time (in hundredths of a second) since the controller was last re-initialized.
Number of Ports | The number of L2 ports in the controller.
L2 Switch MAC Address | The MAC address of the Layer 2 switch in the controller.
Ethernet Chip Information | Ethernet Chip Count | The number of BCM Ethernet chips in the controller.
BIST Status | The status of the Ethernet chip Built-in Self-Test (BIST). The status is a bit-based value: 0x00 - No failure 0x01 - Buffer control RAM (only in BCM5380M) 0x02 - Internal packet data buffer memory 0x04 - MIB RAM (only in BCM5380M) 0x08 - Gigabit MIB RAM (only in BCM5380M)
Rev. ID | Ethernet chip revision ID.
Type | Ethernet chip type: BCM5380M (1) BCM5325E (2) Other (3)

## Example:

### Entry: L2 STATUS SWITCH

System Response:

LAYER 2 SWITCH:

+-------------------------------+------------------+

| Uptime (sec) | 47280 |

| Number of Ports | 11 |

| Switch Manager... | |

| IP Address | 10.37.188.10 |

| MAC Address | 08000f1b3ef8 |

| Chip Count | 1 |

|-------------------------------+------------------|

| Ethernet Chip Information: | |

| BIST Status | 00 |

| Revision ID | A2 |

| Type | |

+-------------------------------+------------------+