# Voice Quality Monitoring

## Purpose

The Voice Quality Monitoring form is used to enable or disable voice quality monitoring. Use this form when performing the following tasks:

- Voice Quality Monitoring

For more information:

- Voice Quality Statistics

## Field Descriptions

Parameter | Description | Default Value
Voice Quality Monitoring | This field allows you to turn voice quality monitoring on (true) or off (false) for all voice quality capable sets registered with this MiVoice Business system. | Disabled
Voice Quality SNMP Trap - Latency Threshold | Sets the threshold for triggering an SNMP trap to warn MiVoice Business or other management application of excessive voice packet delay in the network. Range 0 to 65535 milliseconds. | 9999 ms