# MOVE SWAP

## Qualifiers:

<first number > WITH <second number>

## Purpose:

Allows two users to swap telephones.

## Details:

The following attributes are swapped in the Move Swap operation:

- Name, department, and location

- Directory number

- Interconnect number

- Default account code

- Class or Service information

- Class of Restriction information

- Personal speedcall information

- Hunt group pilot number

- Button speed calls

- Call forward settings

- Do not disturb

- Auto answer.

NOTES

- The MOVE SWAP command does not move Message waiting indications. Before using the command, you should delete any messages (Callback or Dialed) from the set.

- When a device is moved from one call group to another, its Group Presence status is reset to the default presence status of the new group and its members.

You cannot invoke the MOVE SWAP command against the following devices:

- ONS devices programmed as Night Bells

- ONS/OPS devices assigned as Recorded Announcement Devices

- Telephones programmed as Hotel Extensions

- IP Devices.

You cannot use the MOVE SWAP command unless the device types are the same on both ports.

## Example:

### Entry: MOVE SWAP 3000 WITH 3001

System Response:

Operation successful.