# Analog Services Units

## Purpose

The Analog Services Units form defines the analog services units that are supported by the system.

Use this form to perform the following tasks:

- Program an ASU

- Program an ASU II

- Program a Universal ASU

- Program Embedded Analog

- Program Analog Sets and Trunks on an AX

- Program Analog Telephones

## Field Descriptions

Parameter | Description | Default Value
Controller Module | System-generated, protected field that identifies the controller module slot locations. For embedded analog cards and onboard Copper Interface Modules (CIMs) this field displays a dash (-). For Quad CIM modules, this field lists the slot number of the module. |
Port | System-generated, protected field that identifies the purpose of the port. For systems with an embedded analog card, the Programmed Type for Port 0 is "3300 Embedded Analog" or "3300 Expanded Analog". For the AX controller, the Programmed Type field for Port 1 is "AX Card Chassis". For systems that have an external ASU that is connected through an embedded CIM or a Quad CIM, this field displays the Port ID of the CIM through which the ASU is connected. CIM ports are numbered from left to right. Embedded CIM ports or Quad CIM ports can be set as "Not Supported", "3300 Universal ASU", "ASU", or "ASU II". On a CX II or CXi II platform, the fourth port on each Quad CIM module is not supported and, the Installed Type field for these ports always displays "Port Not Supported". |
Unit | Enter a unit number from 2 through 16. | Blank
Programmed Type | Select the programmed unit type. | Not programmed
Installed Type | System-generated, protected field. Identifies the installed unit type. |
Comment | Enter any applicable comments (optional) up to 14 alphanumeric characters long. | Blank
Programmed Card Slot 1 | For the ASU II only. Select the card type. | Not programmed
Installed Card Slot 1 | For the ASU II only. System-generated, protected field. Identifies the installed card type. |
Programmed Card Slot 2 | For the ASU II only. Select the card type. | Not programmed
Installed Card Slot 2 | For the ASU II only. System-generated, protected field, Identifies the installed card type. |