# Speed Call - Personal

## Description

Personal Speed Calls let you store and dial frequently-used numbers by using access codes and index numbers.

## Conditions and Feature Interactions

- The number of Speed Call users cannot exceed 500. Speed Call Digit String (average 12 digits) cannot exceed 1500.

- Each user can be assigned a maximum of 100 Personal Speed Calls (00 to 99) in blocks of 10. If you are assigned 20 Speed Calls, you use index numbers 00 to 19.

- Speed Call index numbers must be two-digit numbers from 00 to 99. If you enter a one or a three-digit index number followed by the speed call number, the system will interpret the first two digits as the index number and the following digits as the speed call number. For example, if you enter "1" as the index number followed by "592-2122", the system will save "92-2122" for index 15. Likewise, if you enter "100" as the index number followed by "592-2122", the system will save "0-592-2122" for index 10.

- You can store up to 26 digits per Speed Call.

- Personal Speed Calls cannot override interconnect restrictions.

- You do not have to enter all of the directory number digits into the Index memory location. For example, if you have an external account code, you can Speed Call the long distance number and manually dial the external account code.

- You can insert a Trunk Flash into a Speed Call. See Flash - Trunk for more details.

## Programming

1. Personal Speed Call Allocation form

- Assign a block of personal speed call numbers to the station (up to 100 in multiples of 10).

2. Feature Access Codes form

Assign Feature Access codes for the following features:

- Personal Speed Call - Invoke

- Personal Speed Call - Store

- Personal Speed Call - Remove

3. To assign a Personal Speed Call key on a 5302 SIP Phone see, Programming Speed Call Keys on a 5302 SIP Phone.

## Device Support

- Supported on all devices.

## Operation

NOTE: Index numbers must be two-digit numbers within your assigned range (00 to a maximum of 99). If you are assigned 20 Speed Calls, use index numbers 00 to 19 when storing Speed Calls. For numbers 0 to 9, add a leading zero. (For example, 00, 01, 02, 03 and so on.)

#### Mitel and 2500 telephones

To dial a Speed Call number:

1. Lift the handset.

2. Dial the Personal Speed Call-Invoke feature access code.

3. Enter a personal speed call index number.

To store a Speed Call number:

1. Lift the handset.

2. Dial the Personal Speed Call-Store feature access code.

3. Enter a two-digit personal speed call index number (from 00 to a maximum of 99).
   For numbers 0 to 9, add a leading zero. (For example, 00, 01, 02, 03 and so on.)

4. Dial the number to be stored.

5. Hang up.

#### Symbol NetVision Phone

To dial a Speed Call number:

1. Press SND.

2. Dial the Personal Speed Call-Invoke feature access code.

3. Enter a personal speed call index number.

To store a Speed Call number:

1. Press SND.

2. Dial the Personal Speed Call-Store feature access code.

3. Enter a two-digit personal speed call index number (from 00 to a maximum of 99).
   For numbers 0 to 9, add a leading zero. (For example, 00, 01, 02, 03 and so on.)

4. Dial the number to be stored.

5. Press END.

#### Symbol MiNET Wireless Phone

To dial a Speed Call number:

1. Press the Send Key.

2. Dial the Personal Speed Call-Invoke feature access code.

3. Enter a personal speed call index number.

To store a Speed Call number:

1. Press the Send Key.

2. Dial the Personal Speed Call-Store feature access code.

3. Enter a two-digit personal speed call index number (from 00 to a maximum of 99).
   For numbers 0 to 9, add a leading zero. (For example, 00, 01, 02, 03 and so on.)

4. Dial the number to be stored.

5. Press the End Key.

#### OpenPhone 27

To dial a Speed Call number:

1. Press .

2. Dial the Personal Speed Call-Invoke feature access code.

3. Enter a personal speed call index number.

To store a Speed Call number:

1. Press .

2. Dial the Personal Speed Call-Store feature access code.

3. Enter a two-digit personal speed call index number (from 00 to a maximum of 99).
   For numbers 0 to 9, add a leading zero. (For example, 00, 01, 02, 03 and so on.)

4. Dial the number to be stored.

5. Press to hang up.

#### SpectraLink Wireless Telephones

To dial a Speed Call number:

1. Press .

2. Dial the Personal Speed Call-Invoke feature access code.

3. Enter a personal speed call index number.

To store a Speed Call number:

1. Press .

2. Dial the Personal Speed Call-Store feature access code.

3. Enter a two-digit personal speed call index number (from 00 to a maximum of 99).
   For numbers 0 to 9, add a leading zero. (For example, 00, 01, 02, 03 and so on.)

4. Dial the number to be stored.

5. Press .

Related Topics

- Flash - Trunk

- Speed Call - Pause

- Speed Call - System

- Speed Call Keys