# Analog Media Gateway AX Controller

In a clustered configuration, you can configure the AX controller as an analog media gateway. As an analog media gateway, the AX Controller does not support any on-board digital trunking. Network access is provided via another MiVoice Business system as an access point.

In an analog media gateway configuration, you can manage the AX controller either

- remotely through the embedded remote management feature of the main office ICP, or

- locally through the System Administration Tool of the AX controller.

Analog Media Gateway AX Controller

Related Topics

- About the AX Controller

- Standalone AX Controller

- Program Analog Sets and Trunks on an AX Controller