# Programming Symbol NetVision MiNET Phones

## Before You Begin

Ensure the following is complete:

- Program Class of Service, Interconnect Restriction, and Intercept Handling.

- Install the Symbol NetVision MiNET Phone Administrator Tool on a Windows NT or Windows 2000 PC.

## Programming

To program a Symbol NetVision MiNET Phone:

1. Wireless IP Sets form

Enter the following information:

- Directory Number (DN)

- PIN Number (must be four digits)

- ACD Set

- Interconnect Number

- Tenant Number

2. (Optional) Default Account Codes form

3. Create a default account code number that will appear in all SMDR records for the station.

3. Station Attributes form

- Assign a Class of Service, Class of Restriction, and Intercept Number to the DN of the phone.

- (Optional) Assign a Default Account Code Index number.

4. User and Services Configuration form

- Use the User and Services Configuration search field to locate the directory number that you assigned to the device. Assign a name, department, and location to the directory number.

5. Update the NetVision MiNET Phone to use the MiNET protocol.

   NOTE: For easy access to the various Mitel documentation suites go to Document Center.

6. Import the MitelWM.csv file from MiVoice Business to the NetVision MiNET Phone Administrator Tool.

7. Perform a firmware upgrade, either manually or automatically.

NOTE: To automatically update the NetVision MiNET Phone's firmware, you must configure the AirBEAM parameters. AirBEAM is a feature available through the NetVision MiNET Phone Administrator Tool that allows automatic download of phone firmware and configuration data to wireless phones.

8. Create profiles for the NetVision MiNET phone.

9. Download the profiles to the NetVision MiNET Phone.

NOTE: If you delete telephones, you must also delete the corresponding directory entries and voice mailboxes.