# Call Privacy - Tone and Intrusion Suppression

## Description

This feature protects a call from interruptions. When activated, Call Privacy - Tone and Intrusion Suppression ensures that you do not receive any audible camp-on tones, and prevents intrusion of any kind (for example, Busy Override). The user activates Call Privacy by dialing a Feature Access Code (FAC) immediately prior to the call, or during a call (after temporarily placing the other party on hold). Call Privacy remains effective for the duration of the call.

## Conditions and Feature Interactions

None

## Programming

1. Class of Service Options form

- For Call Privacy only, enable the COS option "Call Privacy" in the Class of Service of the station which is to be secured from intrusion during a call.

2. Feature Access Codes form

3. Assign a Feature Access code to the Call Privacy feature.

## Device Support

- Supported on all devices.

## Operation

#### Mitel and 2500 telephones

To enable Call Privacy - Tone and Intrusion Suppression before dialing a destination:

1. Lift handset.

2. Dial the Caller Privacy feature access code.

3. Dial the destination number.

#### Symbol NetVision Phone

To enable Call Privacy - Tone and Intrusion Suppression before dialing a destination:

1. Press SND.

2. Dial the Caller Privacy feature access code.

3. Dial the destination number.

#### Symbol MiNET Wireless Phone

To enable Call Privacy - Tone and Intrusion Suppression before dialing a destination:

1. Press the Send Key.

2. Dial the Caller Privacy feature access code.

3. Dial the destination number.

Related Topics

- Call Privacy - Name and Number Suppression