# Adding an External Music on Hold Source to an AX

## Overview

The SX-200 Music On Hold Input Adapter (PN 50006162) allows you to connect an external audio device (e.g., a radio) to a 3300 AX and use it as the system MOH source. To bypass the embedded MOH, you use the Tenant feature and configure the external device as the MOH source for Tenant 1.

## Programming

To add an External Music on Hold Source to an AX:

1. Connect the MOH audio source to an ONS card in the AX as shown:

Click image to enlarge

2. Tenants form

- select External as the Audio Source

- enter the DN of ONS port as the Music on Hold Music Source..

3. Reboot the system..

Related Topics

- Music on Hold

- Music on Hold On Transfer