# Hot Desk Logout

To log out from a hot desk set, invoke log out by entering a feature access code (FAC) or pressing a softkey. After you log out (or are logged out by the system), your DN follows out-of-service handling and the hot desk set reverts back to the programming associated with its profile.

To log out a hot desk set immediately, the prime line must be idle (no ringing, active, or held call). You are able to logout immediately even if you have non-prime lines that are in a ringing, flashing, or in use by other co-workers.

Depending on your set type, you initiate a Hot Desk logout when the prime line is idle by

- Pressing the "Logout" softkey

- Pressing the Hot Desking feature key and then press the "Logout" softkey

- Dialing the hot desk Logout FAC (Feature Access Code)

- Dialing the hot desk Remote Logout FAC followed by the DN of the idle hot desk user

To initiate a logout while the prime line is busy on a call (delayed logout)

- Press the "Hot Desking" feature key, and then press the " Logout" softkey. Logout occurs when the prime line returns to idle state.

The following conditions apply to hot desk logout:

- Delayed logout functionality is not supported for traditional ACD agents, but is supported for Hot Desk ACD agents.

- If you are busy or have a call on hold on any line, you can still initiate a logout. After the hot desk set returns to idle state, your logout takes effect.

- Both traditional ACD agents and hot desk ACD agents can logout while their non-prime lines are ringing. After hot desk agents logout, calls on their non-prime lines will not get answered unless they are ringing on another device, or get diverted to another device.

- If a device's prime line is being rung, then the logout attempt is rejected.

- An administrator with remote logout permission can log out a user remotely using the Remote Logout access code and the user's DN.

Hot desk sets can also be logged out automatically using the Scheduler.

NOTE: When a resilient hot desk device rehomes to a switch that has a newer device firmware, the user (including hot desk ACD agents) is automatically logged out to allow the firmware upgrade to proceed.

## Hot Desk Auto Logout

Hot desk users can be automatically logged out after a preset duration. To log out a hot desk user automatically, set the duration (in hours) in the Hot Desk Auto Logout Timer Class of Service (COS) option. When Hot Desk Auto Logout Timer expires, the hot desk user is automatically logged out.

The hot desk auto logout is supported for the following hot desk users:

- MiNet Hot Desk

- External Hot Desk User (EHDU)

- SIP Hot Desk

- ACD Hot Desk

- External Hot Desk Agent (EHDA)

NOTE: Hot desk auto logout is not supported for traditional ACD agents.

The following conditions apply to hot desk auto logout feature:

- This feature applies irrespective of whether hot desk users are active or inactive.

- If an EHDU does not have a permanent login COS, then the feature applies to the EHDU regardless whether logged into the PSTN, MiNet or SIP.

- If an EHDU has a permanent login COS, then the feature is applied when the EDHU is logged into MiNet or SIP.

- A EHDU with a permanent login COS, when changes the logon location from a PSTN to non-PSTN and vice-versa, the system considers this as a logout and login, and restarts the logon duration.

- If Hot Desk Auto Logout Timer expires while a hot desk user is still busy on a call, the log out occurs when the hot desk user returns to idle state.

- Hot desk users' logon duration is maintained on primary and secondary servers during failovers and fallbacks. As a prerequisite, both the primary and secondary servers must on MiVB 8.0 SP1 release.

- The hot desk users' logon duration is stored on a volatile memory. This information is lost when the system is rebooted.

- When an active hot desk user (logged into a telephone) logs into another telephone, the logon duration is carried forward from the first telephone to the second telephone (this is, the system does not consider this as a logout and login).

- When two hot desk users are logged into the same telephone, if the first hot desk user logs out, the system clears the logon information of the first hot desk user and starts the timer for the second hot desk user.

- During an active Mobile Line call, the Hot Desk Auto Logout Timer expires and disables the Mobile Line feature. The call is transferred to the mobile phone.

5005 IP Phone, 5205 IP Phone, and 5207 IP Phone

- Dial the Hot Desking Logout access code.

5010 IP Phone, 5212 IP Phone, 5215 IP Phone and 5215 IP Phone (Dual Mode), 5304 IP Phone, and 5312 IP Phone

1. Dial the Hot Desking Logout access code.

2. Press #.

5020 IP Phone, 5220 IP Phone, 5220 IP Phone (Dual Mode), 5224 IP Phone, 5324 IP Phone, and Navigator

1. Press the Logout softkey.

2. Press the Logout softkey again to confirm.

5320 IP Phone, 5330/5330e IP Phone, 5340/5340e IP Phone, 5360 IP Phone, and 69xx IP Phones

To log out of Hot Desking phone (the phone must be idle):

1. Press the key you have programmed to HotDesking.

2. Press the Logout softkey.

3. Press the Confirm softkey.

NOTE: Your profile can only be active on one phone at a time. If you log in from another phone without logging out from the first one, the system will automatically deactivate your profile on the first phone.

To remotely log out a Hot Desking phone (this feature must be allowed by your System Administrator through the Class of Service:

1. Using the phone keys, dial the appropriate feature access code.

2. Using the phone keys, dial the Hot Desk User Extension Number that you want to log out.

3. Press the Logout softkey.

4. Press the Confirm softkey.

5560 IPT

1. Press the Menu key.

2. Press the Logout key.

5140 IP Phone and 5240 IP Phone

1. From the Phone View screen, press the HotDesk softkey.

2. Press the Logout softkey.

3. Press the Logout softkey again to confirm.

SpectraLink Wireless Telephones

1. Press the Logo softkey.

2. Press the Logo softkey again to confirm.

5604, 5607, 5614 Wireless Phones

1. Press the END CALL key and hold it until the Logout pop-up window is displayed.

2. Press the YES softkey to log out. (Pressing NO cancels the logout request.)

Mitel SIP-DECT Phones (models 612, 622, 632, and 650)

1. Dial the Hot Desking Logout access code followed by #.

OR

2. Press until the System Menu opens.

3. Select Administration.

4. Select User logout.

5. Enter User PIN.

Remote logout (all devices)

1. Dial the Remote Logout access code.

2. Enter the hot desk user DN.

Related Topics

- Hot Desking Description

- Hot Desking Conditions

- Hot Desking Programming

- Program Nodal Hot Desking

- Program Clustered Hot Desking

- Hot Desking Login

- Hot Desking PIN Change

- Hot Desking Troubleshooting

- Scheduling Hot Desk User Logouts

- Hot Desk PIN Security