# Controller Module Configuration

## Purpose

The Controller Module Configuration form identifies the modules that are in the controller.

NOTE: The EX controller does not support the Controller Module.

Use this form to perform the following tasks:

- Program Controller Modules

- Program Embedded BRI Trunks

- Program Embedded PRI/QSIG Trunks

- Program Embedded T1/D4 Trunks

- Program a MiVoice Business System as a Standalone Voice Mail Server

## Field Descriptions

Parameter | Description | Default Value
Module | System-generated, protected field. Indicates the module position in the controller. |
Programmed Module Type | For the MXe III controllers, select ", "Dual Framer", "T1/E1", "Quad BRI", or "Quad CIM" to match the Installed Module Type. For the CX II or CXi II controller, you can select "T1/E1", "Quad BRI", or "Quad CIM". For the AX controller, you can select "Dual Framer", "T1/E1", or "Quad BRI". You can install a maximum of two Quad CIM modules in a MiVoice Business controller with the exception of the AX controller which only supports one Quad CIM module. A Quad CIM module provides 4 ports. You can connect an ASU, a Universal ASU, or an ASU II to a Quad CIM port. NOTE On the CXi II controller, only the first three ports on each Quad CIM are functional — the fourth port is not supported. | No Module Programmed
Installed Module Type | System-generated, protected field. Indicates the type of module installed in the specified location. |