# EDT TRACE

## Qualifiers:

TSP L2L3 <cabinet> <shelf> <slot> <port>

TSP CC <cabinet> <shelf> <slot> <port>

TSP MTCE

TSP SRVC

VDSU <UAPI, CP, VB, NAMNUM> <cabinet> <shelf> <slot> <port>

## Purpose:

The TRACE command toggles the display of messages that pass through the system. Each time you issue the TRACE command it turns message display on or off and updates the state of the command on the hard drive. The state (on or off) of the TRACE command is maintained after a system reset.

NOTE: The TRACE command is used to collect data for interpretation by Mitel technical support. The data is not meant to be interpreted by customers or field technicians.

## Definitions:

Trunk Service Provider (TSP) - The protocol stack for that trunk type (typically provides layer2/3 information)

## Details:

TSP L2L3 qualifier outputs the Layer 2 or Layer 3 switch traces for the PRI, QSIG, and BRI trunks.

TSP CC qualifier toggles the SP Call Control verbose message traces.

TSP MTCE qualifier toggles SP Maintenance verbose message trace.

TSP SRVC qualifier toggles SP Service verbose message trace.

VDSU UAPI qualifier toggles tracing between the Trunk Service Provider and the VDSU.

VDSU CP qualifier toggles Call Processing message tracing.

VDSU VB qualifier toggles Verbose message tracing. Note that you must enable VDSU CP message tracing before you can enable Verbose message tracing.

VDSU NAMNUM qualifier toggles the output of the called party number, calling party number, calling name, and disconnect cause reason on a per call basis.

Use the EDT ENABLE LOGTOFILE command to save the logging traces to a file named "LDS_Trace.rtf" in the "/db" directory. This log file must be interpreted by Mitel Design. It is not meant to be interpreted by field technicians.

## Examples:

### Entry: EDT TRACE TSP L2L3 8 1 2 1

System Response:

2005-04-06 09:56:05 HDLC CC on link 3 trace enable .
2005-04-06 09:56:05 HDLC VERBOSE on link 3 trace enable .

Enter the command again to disable:

2005-04-06 09:56:21 HDLC CC on link 3 trace disable .
2005-04-06 09:56:21 HDLC VERBOSE on link 3 trace disable .

### Entry: EDT TRACE TSP CC 8 1 2 1

System Response:

2005-04-06 08:34:46 CC UP on link 3 trace enable .
2005-04-06 08:34:46 CC DOWN on link 3 trace enable .
2005-04-06 08:34:46 CC VERBOSE on link 3 trace enable .

Enter the command again to disable:

2005-04-06 08:36:05 CC UP on link 3 trace disable .
2005-04-06 08:36:05 CC DOWN on link 3 trace disable .
2005-04-06 08:36:05 CC VERBOSE on link 3 trace disable .

### Entry: EDT TRACE VDSU UAPI 8 1 2 1

System Response:

2005-04-06 08:44:28
Uapi Message Tracing Toggled
2005-04-06 08:44:28
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
UAPI
PRINTF

Enter the command again to disable:

2005-04-06 08:54:19
Uapi Message Tracing Toggled
2005-04-06 08:54:19
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
All debug flags are off

### Entry: EDT TRACE VDSU CP 8 1 2 1

System Response:

2005-04-06 08:55:21
CP Message Tracing Toggled
2005-04-06 08:55:21
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
CP
PRINTF

Enter the command again to disable:

2 005-04-06 08:56:10
CP Message Tracing Toggled
2005-04-06 08:56:10
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
All debug flags are off

### Entry: EDT TRACE VDSU VB 8 1 2 1

System Response:

2005-04-06 08:56:40
VB Message Tracing Toggled
2005-04-06 08:56:40
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
VERBOSE
PRINTF

Enter the command again to disable:

2005-04-06 08:57:14
VB Message Tracing Toggled
2005-04-06 08:57:14
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
All debug flags are off

### Entry: EDT TRACE VDSU NAMNUM 8 1 2 1

System Response:

2005-04-06 08:58:37
NAMNUM Message Tracing Toggled
2005-04-06 08:58:37
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
NAM NUM
PRINTF

Enter the command again to disable:

2005-04-06 08:59:18
NAMNUM Message Tracing Toggled
2005-04-06 08:59:18
Debug trace(s) enabled on ISDN VDsu Mod 2 Port 1
All debug flags are off