# Analog Sets

## Purpose

The Analog Sets form is used to assign directory numbers, circuit descriptor numbers, and interconnect numbers to ONS circuits.

Use this form to perform the following tasks:

- Program Analog Telephones

- Program Analog Sets and Trunks on an AX

- Program Analog Sets on an EX Controller

- Program a 3300 Universal ASU

- Program a ASU II

- Program a ASU

## Conditions

- When deleting analog sets, you must also delete the corresponding directory entries and voice mailboxes.

## Field Descriptions

Parameter | Description | Default Value
Cabinet | System-generated, protected field. Identifies the physical location. |
Shelf | System-generated, protected field. Identifies the physical location. |
Slot | System-generated, protected field. Identifies the physical location. |
Circuit | System-generated, protected field. Identifies the physical location. |
Card Type | System-generated, protected field. Identifies the card type. |
Number | Enter a unique directory number (not assigned to any other device, hunt group, or feature access code) for the line circuit. Can be up to 1 to 7 digits in length. | Blank
Local-only DN | Allows you to specify the directory number as a local-only directory number in a cluster. See Local-only Directory Numbers and RDN Synchronization for more information. | Not Selected
Circ. Desc. Index | Enter the circuit descriptor number that defines the operational parameters of the line circuit (from the ONS/OPS Circuit Descriptors form). | Blank
Interconnect Number | Enter a number which will be used in the Interconnect Restriction form to define which other devices can connect to the ONS line. Can be in the range of 1 and the upper limit. | Blank
Non-Busy Ext. | Select "Yes" to indicate that the associated extension is a non-busy extension ( NBE). A NBE will never return a busy tone to the caller; each caller will automatically intrude and form a conference with any other users. Up to eight users may be conferenced together, and further calls are queued and allowed to enter the conference as current members drop out. The NBE cannot originate calls unless it is also programmed as a hotline extension. NOTE: A non-busy extension requires a COS that has the conference option enabled. | No
Tenant Number | Enter the number of the set's tenant. | 1 (landlord)
User PIN | Enter a password for the user PIN. The PIN can only include digits from 0 to 9 and can be from 0 to 8 digits in length. | Blank
Confirm User PIN | Re-enter the password to confirm that it was correctly entered in the User PIN field. | Blank
Service Level | System-generated, protected field. Identifies the Service Level assigned to the device in the User and Services Configuration form. NOTE: All devices added on this form have Full Service This Service Level indicates that the directory number (DN) is assigned to a standard user and device with full telephony functionality.. Use the User and Services Configuration form to program other Service Levels. |
Remote Group Pilot Number | Enter a valid prime directory number up to seven digits in length to be used as the pilot number for the Suite EHDU. The pilot number is the number dialed to access the suite. See Centralized Suites for Analog Devices for details. | Blank